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Benchmarks

For the purposes of this Annex, the definitions of products covered and of processes and emissions covered (system boundaries) set out in Annex I to Delegated Regulation (EU) 2019/331 shall apply. 
1. Product benchmarks without collection of data on electricity consumption 
	Product benchmark
	Average value of the 10% most efficient installations in 2021 and 2022 (t CO2 equivalents/t)
	Benchmark value (allowances/t) for 2026-2030

	Coke
	0,132
	0,143

	Agglomerated iron ore
	0,024
	0,086

	Hot metal
	1,360
	1,248

	Pre-bake anode
	0,300
	0,290

	Aluminium
	1,489
	1,423

	Grey cement clinker
	0,689
	0,656

	White cement clinker
	0,919
	0,890

	Lime
	0,771
	0,693

	Dolime
	0,876
	0,792

	Sintered dolime
	1,248
	1,162

	Float glass
	0,412
	0,394

	Bottles and jars of colourless glass
	0,284
	0,242

	Bottles and jars of coloured glass
	0,255
	0,233

	Continuous filament glass fibre products
	0,284
	0,232

	Facing bricks
	0,100
	0,083

	Pavers
	0,133
	0,108

	Roof tiles
	0,128
	0,121

	Spray-dried powder
	0,055
	0,046

	Plaster
	0,049
	0,045

	Dried secondary gypsum
	0,010
	0,009

	Short fibre kraft pulp
	0,029
	0,060

	Long fibre kraft pulp
	0,046
	0,040

	Sulphite pulp, thermo-mechanical and mechanical pulp
	0,000
	0,010

	Recovered paper pulp
	0,000
	0,020

	Newsprint
	0,018
	0,149

	Uncoated fine paper
	0,015
	0,159

	Coated fine paper
	0,066
	0,159

	Tissue
	0,170
	0,167

	Testliner and fluting
	0,056
	0,124

	Uncoated carton board
	0,021
	0,119

	Coated carton board
	0,034
	0,137

	Nitric acid
	0,015
	0,151

	Adipic acid
	0,34
	1,40

	Vinyl chloride monomer (VCM)
	0,195
	0,191

	Phenol/acetone
	0,233
	0,219

	S-PVC
	0,082
	0,080

	E-PVC
	0,184
	0,161

	Soda ash
		0,748
	1,122



Product benchmarks with collection of data on electricity consumption
	Product benchmark
	Average value of the 10% most efficient installations in 2021 and 2022 (t CO2 equivalents/t)
	Benchmark value (allowances/t) for 2026-2030

	Refinery products
	0,0251
	0,0232

	EAF carbon steel
	0,130
	0,142

	EAF high alloy steel
	0,186
	0,176

	Iron casting
	0,210
	0,163

	Mineral wool
	0,413
	0,341

	Plasterboard
	0,125
	0,122

	Carbon black
	1,320
	1,048

	Ammonia
	1,630
	1,522

	Steam cracking
	0,657
	0,638

	Aromatics
	0,0116
	0,0232

	Styrene
	0,318
	0,264

	Hydrogen
	8,24
	7,98

	Synthesis gas (syngas)
	0,002
	0,190

	Ethylene oxide/ethylene glycols
	0,378
	0,321



Heat and fuel benchmarks
	Benchmark
	Average value of the 10% most efficient installations in 2021 and 2022 (t CO2 equivalents/TJ)
	Benchmark value (allowances/TJ) for 2026-2030

	Heat benchmark
	7,2
	31,2

	Fuel benchmark
	10,4
	28,1





EN	0		EN
image1.emf
   

 EUROPEAN   COMMISSION   

Brussels,  XXX     […] (2026)  XXX   draft   ANNEX     ANNEX   to the   Commission Implementing Regulation (EU) .../...   determining revised benchmark values for free allocation of emission allowances for the  period from 2026 to 2030 pursuant to Article 10a(2) of Directive 2003/87/EC of the  European Parliament and of the Council  


